20 40 60 80 100

0 1 2 3 4 5

Ο 1 track Ο 2 tracks Ο 3 tracks

2 additional minbias events overlayed (a)

Efficiency (Ψ)

20 40 60 80 100

0 1 2 3 4 5

Ο 1 track Ο 2 tracks Ο 3 tracks

5 additional minbias events overlayed (b)

S_{min}

Efficiency (Ψ)