Figure 6: Relative signal trigger efficiency as a function of trigger rate for the trigger based on requiring at least N STT tracks above some |b|_{max} threshold. Each curve corresponds to a different threshold. The curve which gives the best overall performance corresponds to |b_{max}| ≥ 30.0 μm.